# Raspberry Pi LoRa KISS TNC

This project was originally started by Tom Kottek (https://github.com/tomelec/RPi-LoRa-KISS-TNC). Because the program had some problems dealing with digipeated frames (it crashed when receiving a ssid with the 'has_been_digipeated' flag -*- set), I took on the task of fixing the code for my personal use.

## Hardware

I also designed my own (open source) hardware for it: a board holding a Raspberry Pi Zero 2 W, an SX1278 LoRa transceiver and a power supply with on/off button to safely switch on and off the system. The design files can be found on my website: [RPi LoRa_shield](https://meezenest.nl/mees/RPi_LoRa_shield.html)

## Software

The software controls the LoRa transceiver connected to the Raspberry´s SPI bus and emulates a KISS TNC over TCP. That makes it possible to use existing software like APRX. It is also possible to attach the KISS interface to the AX.25 stack via socat/kissattach.

### To Do
* A lot
