(export (version D)
  (design
    (source /home/marcel/Documenten/electronische_projecten/lora-kiss-tnc-pico/lora_kiss_tnc_pico_KiCad_rev2/lora_kiss_tnc_pico_rev2.sch)
    (date "ma 25 apr 2022 13:59:41 CEST")
    (tool "Eeschema 5.1.8-5.1.8")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "LORA KISS TNC Pico")
        (company "M. Konstapel")
        (rev 2)
        (date 2022-04-25)
        (source lora_kiss_tnc_pico_rev2.sch)
        (comment (number 1) (value https://meezenest.nl/mees))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value Ra-02)
      (footprint mtk_rf:RA-02)
      (fields
        (field (name Manufacturer) Thinker)
        (field (name "Ordering #") Ra-02))
      (libsource (lib mtk_rf) (part Ra-02) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61E5E459))
    (comp (ref D6)
      (value "Dual LED")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "Pin header 1x3 2.54mm"))
      (libsource (lib Device) (part LED_Dual_ACA) (description "Dual LED, common cathode on pin 2"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EA59A8))
    (comp (ref R7)
      (value 470R)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "470R 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EB5A7D))
    (comp (ref R6)
      (value 470R)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "470R 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EBD1AF))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "100n/50V 5mm"))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F5371B))
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10k 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EEB42A))
    (comp (ref R5)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10k 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61EEB432))
    (comp (ref H1)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_DIN965_Pad)
      (datasheet ~)
      (fields
        (field (name Manufacturer) "Not a placeable part")
        (field (name "Ordering #") -))
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6200BDDD))
    (comp (ref H2)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_DIN965_Pad)
      (datasheet ~)
      (fields
        (field (name Manufacturer) "Not a placeable part")
        (field (name "Ordering #") -))
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6200C56C))
    (comp (ref H3)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_DIN965_Pad)
      (datasheet ~)
      (fields
        (field (name Manufacturer) "Not a placeable part")
        (field (name "Ordering #") -))
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6200C756))
    (comp (ref H4)
      (value M3)
      (footprint MountingHole:MountingHole_3.2mm_M3_DIN965_Pad)
      (datasheet ~)
      (fields
        (field (name Manufacturer) "Not a placeable part")
        (field (name "Ordering #") -))
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6200C9C8))
    (comp (ref U2)
      (value Pico)
      (footprint MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH)
      (fields
        (field (name Manufacturer) "Raspberry Pi")
        (field (name "Ordering #") Pico))
      (libsource (lib MCU_RaspberryPi_and_Boards) (part Pico) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F073D4))
    (comp (ref U3)
      (value LD1117S33)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000544.pdf)
      (fields
        (field (name "Conrad #") "147028 - 62")
        (field (name Manufacturer) STMicroelectronics)
        (field (name "Ordering #") LD1117V33))
      (libsource (lib Regulator_Linear) (part LD1117S33TR_SOT223) (description "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 3.3V, SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F0B69A))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "100n/50V 5mm"))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F5F4DC))
    (comp (ref C3)
      (value 10U/10V)
      (footprint Capacitor_THT:CP_Radial_D6.3mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10U/25V 2.5mm"))
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F600EA))
    (comp (ref D1)
      (value LED)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "Pin header 1x2 2.54mm"))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F66A16))
    (comp (ref R3)
      (value 470R)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "470R 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F69333))
    (comp (ref Q1)
      (value BC557)
      (footprint Package_TO_SOT_THT:TO-92_Wide)
      (datasheet http://www.fairchildsemi.com/ds/BC/BC557.pdf)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") BC557))
      (libsource (lib Transistor_BJT) (part BC557) (description "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F6F7AD))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10k 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F80339))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10k 1% 0.25W"))
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F80342))
    (comp (ref Q2)
      (value BC557)
      (footprint Package_TO_SOT_THT:TO-92_Wide)
      (datasheet http://www.fairchildsemi.com/ds/BC/BC557.pdf)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") BC557))
      (libsource (lib Transistor_BJT) (part BC557) (description "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61F8034B))
    (comp (ref C4)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "100n/50V 5mm"))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 620424A5))
    (comp (ref J1)
      (value I2C)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "Pin header 1x4 2.54mm"))
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6205372A))
    (comp (ref D2)
      (value SB130)
      (footprint Diode_THT:D_DO-15_P10.16mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name "Conrad #") "164828 - 62")
        (field (name Manufacturer) Vishay)
        (field (name "Ordering #") SB130))
      (libsource (lib Device) (part D_Schottky_Small_ALT) (description "Schottky diode, small symbol, filled shape"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62669DFF))
    (comp (ref J3)
      (value 8-24V)
      (footprint Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical)
      (datasheet ~)
      (fields
        (field (name "Conrad #") "1327243 - 62")
        (field (name Manufacturer) Degson)
        (field (name "Ordering #") DG381-3.5-02P-14-00AH-1))
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6266BA36))
    (comp (ref J2)
      (value GPIO)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "Pin header 1x8 2.54mm"))
      (libsource (lib Connector) (part Conn_01x08_Male) (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 626B251D))
    (comp (ref U4)
      (value TSR_1-2450)
      (footprint Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT)
      (datasheet http://www.tracopower.com/products/tsr1.pdf)
      (fields
        (field (name "Conrad #") "156673 - 62")
        (field (name Manufacturer) TracoPower)
        (field (name "Ordering #") "TSR 1-2450"))
      (libsource (lib Regulator_Switching) (part TSR_1-2450) (description "1A step-down regulator module, fixed 5V output voltage, 5-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6266E2A2))
    (comp (ref C5)
      (value 10U/10V)
      (footprint Capacitor_THT:CP_Radial_D6.3mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "10U/25V 2.5mm"))
      (libsource (lib Device) (part CP_Small) (description "Polarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6267D40F))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Manufacturer) QPL)
        (field (name "Ordering #") "100n/50V 5mm"))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6269954E)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Female)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector) (part Conn_01x08_Male)
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Device) (part CP_Small)
      (description "Polarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky_Small_ALT)
      (description "Schottky diode, small symbol, filled shape")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky_Small_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED_Dual_ACA)
      (description "Dual LED, common cathode on pin 2")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Dual_ACA))
      (pins
        (pin (num 1) (name A1) (type input))
        (pin (num 2) (name K) (type input))
        (pin (num 3) (name A2) (type input))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_RaspberryPi_and_Boards) (part Pico)
      (fields
        (field (name Reference) U)
        (field (name Value) Pico)
        (field (name Footprint) RPi_Pico:RPi_Pico_SMD_TH))
      (pins
        (pin (num 1) (name GPIO0) (type BiDi))
        (pin (num 2) (name GPIO1) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name GPIO2) (type BiDi))
        (pin (num 5) (name GPIO3) (type BiDi))
        (pin (num 6) (name GPIO4) (type BiDi))
        (pin (num 7) (name GPIO5) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name GPIO6) (type BiDi))
        (pin (num 10) (name GPIO7) (type BiDi))
        (pin (num 11) (name GPIO8) (type BiDi))
        (pin (num 12) (name GPIO9) (type BiDi))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name GPIO10) (type BiDi))
        (pin (num 15) (name GPIO11) (type BiDi))
        (pin (num 16) (name GPIO12) (type BiDi))
        (pin (num 17) (name GPIO13) (type BiDi))
        (pin (num 18) (name GND) (type power_in))
        (pin (num 19) (name GPIO14) (type BiDi))
        (pin (num 20) (name GPIO15) (type BiDi))
        (pin (num 21) (name GPIO16) (type BiDi))
        (pin (num 22) (name GPIO17) (type BiDi))
        (pin (num 23) (name GND) (type power_in))
        (pin (num 24) (name GPIO18) (type BiDi))
        (pin (num 25) (name GPIO19) (type BiDi))
        (pin (num 26) (name GPIO20) (type BiDi))
        (pin (num 27) (name GPIO21) (type BiDi))
        (pin (num 28) (name GND) (type power_in))
        (pin (num 29) (name GPIO22) (type BiDi))
        (pin (num 30) (name RUN) (type input))
        (pin (num 31) (name GPIO26_ADC0) (type BiDi))
        (pin (num 32) (name GPIO27_ADC1) (type BiDi))
        (pin (num 33) (name AGND) (type power_in))
        (pin (num 34) (name GPIO28_ADC2) (type BiDi))
        (pin (num 35) (name ADC_VREF) (type power_in))
        (pin (num 36) (name 3V3) (type power_in))
        (pin (num 37) (name 3V3_EN) (type input))
        (pin (num 38) (name GND) (type BiDi))
        (pin (num 39) (name VSYS) (type power_in))
        (pin (num 40) (name VBUS) (type power_in))
        (pin (num 41) (name SWCLK) (type input))
        (pin (num 42) (name GND) (type power_in))
        (pin (num 43) (name SWDIO) (type BiDi))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib Regulator_Linear) (part AP1117-15)
      (aliases
        (alias AP1117-18)
        (alias AP1117-25)
        (alias AP1117-33)
        (alias AP1117-50)
        (alias LD1117S33TR_SOT223)
        (alias LD1117S12TR_SOT223)
        (alias LD1117S18TR_SOT223)
        (alias LD1117S25TR_SOT223)
        (alias LD1117S50TR_SOT223)
        (alias NCP1117-12_SOT223)
        (alias NCP1117-1.5_SOT223)
        (alias NCP1117-1.8_SOT223)
        (alias NCP1117-2.0_SOT223)
        (alias NCP1117-2.5_SOT223)
        (alias NCP1117-2.85_SOT223)
        (alias NCP1117-3.3_SOT223)
        (alias NCP1117-5.0_SOT223)
        (alias AMS1117-1.5)
        (alias AMS1117-1.8)
        (alias AMS1117-2.5)
        (alias AMS1117-2.85)
        (alias AMS1117-3.3)
        (alias AMS1117-5.0))
      (description "1A Low Dropout regulator, positive, 1.5V fixed output, SOT-223")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT?223*TabPin2*))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117-15)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-223-3_TabPin2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Regulator_Switching) (part TSR_1-2450)
      (aliases
        (alias TSR_1-2412)
        (alias TSR_1-2415)
        (alias TSR_1-2418)
        (alias TSR_1-2425)
        (alias TSR_1-2433)
        (alias TSR_1-2465)
        (alias TSR_1-2490)
        (alias TSR_1-24120)
        (alias TSR_1-24150))
      (description "1A step-down regulator module, fixed 5V output voltage, 5-36V input voltage, -40°C to +85°C temperature range, TO-220 compatible LM78xx replacement")
      (docs http://www.tracopower.com/products/tsr1.pdf)
      (footprints
        (fp Converter*DCDC*TRACO*TSR?1*))
      (fields
        (field (name Reference) U)
        (field (name Value) TSR_1-2450)
        (field (name Footprint) Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT))
      (pins
        (pin (num 1) (name Vin) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name Vout) (type power_out))))
    (libpart (lib Transistor_BJT) (part BC557)
      (aliases
        (alias BC556)
        (alias BC558)
        (alias BC559)
        (alias BC560)
        (alias BC327)
        (alias BC328))
      (description "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
      (docs http://www.fairchildsemi.com/ds/BC/BC557.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC557)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name C) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name E) (type passive))))
    (libpart (lib mtk_rf) (part Ra-02)
      (fields
        (field (name Reference) U)
        (field (name Value) Ra-02))
      (pins
        (pin (num 1) (name GND) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name 3V3) (type power_in))
        (pin (num 4) (name RST) (type input))
        (pin (num 5) (name DIO0) (type BiDi))
        (pin (num 6) (name DIO1) (type BiDi))
        (pin (num 7) (name DIO2) (type BiDi))
        (pin (num 8) (name DIO3) (type BiDi))
        (pin (num 9) (name GND) (type passive))
        (pin (num 10) (name DIO4) (type BiDi))
        (pin (num 11) (name DIO5) (type BiDi))
        (pin (num 12) (name SCK) (type BiDi))
        (pin (num 13) (name MISO) (type BiDi))
        (pin (num 14) (name MOSI) (type BiDi))
        (pin (num 15) (name NSS) (type BiDi))
        (pin (num 16) (name GND) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Device)
      (uri /home/marcel/kicad_sources/kicad-symbols-master/Device.lib))
    (library (logical MCU_RaspberryPi_and_Boards)
      (uri "/home/marcel/kicad_sources/KiCad-RP-Pico/RP-Pico Libraries/MCU_RaspberryPi_and_Boards.lib"))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical Regulator_Linear)
      (uri /home/marcel/kicad_sources/kicad-symbols-master/Regulator_Linear.lib))
    (library (logical Regulator_Switching)
      (uri /home/marcel/kicad_sources/kicad-symbols-master/Regulator_Switching.lib))
    (library (logical Transistor_BJT)
      (uri /home/marcel/kicad_sources/kicad-symbols-master/Transistor_BJT.lib))
    (library (logical mtk_rf)
      (uri /home/marcel/Documenten/electronische_projecten/KiCad_libraries/mtk_rf.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref J3) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref U1) (pin 9))
      (node (ref U1) (pin 2))
      (node (ref U1) (pin 16))
      (node (ref U4) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U2) (pin 8))
      (node (ref D1) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 18))
      (node (ref U2) (pin 38))
      (node (ref U1) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 28))
      (node (ref U2) (pin 23))
      (node (ref U3) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 2) (name "Net-(J1-Pad3)")
      (node (ref U2) (pin 31))
      (node (ref J1) (pin 3)))
    (net (code 3) (name "Net-(J1-Pad2)")
      (node (ref U2) (pin 32))
      (node (ref J1) (pin 2)))
    (net (code 4) (name +3V3)
      (node (ref J2) (pin 8))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref C1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Q2) (pin 3))
      (node (ref R5) (pin 1))
      (node (ref J1) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref C4) (pin 1)))
    (net (code 5) (name DIO1)
      (node (ref U2) (pin 12))
      (node (ref U1) (pin 6)))
    (net (code 6) (name LORA_RST)
      (node (ref U2) (pin 15))
      (node (ref U1) (pin 4)))
    (net (code 7) (name "Net-(Q1-Pad1)")
      (node (ref Q1) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 8) (name "Net-(Q2-Pad2)")
      (node (ref Q2) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 9) (name "Net-(D6-Pad3)")
      (node (ref R6) (pin 2))
      (node (ref D6) (pin 3)))
    (net (code 10) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 11) (name "Net-(D1-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 12) (name DCD)
      (node (ref U2) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 13) (name PTT)
      (node (ref U2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 14) (name "Net-(D6-Pad1)")
      (node (ref D6) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 15) (name "Net-(J2-Pad3)")
      (node (ref U2) (pin 5))
      (node (ref J2) (pin 3)))
    (net (code 16) (name "Net-(D2-Pad2)")
      (node (ref U4) (pin 3))
      (node (ref D2) (pin 2)))
    (net (code 17) (name "Net-(C5-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref J3) (pin 1)))
    (net (code 18) (name "Net-(J2-Pad7)")
      (node (ref U2) (pin 10))
      (node (ref J2) (pin 7)))
    (net (code 19) (name "Net-(J2-Pad5)")
      (node (ref U2) (pin 7))
      (node (ref J2) (pin 5)))
    (net (code 20) (name "Net-(J2-Pad4)")
      (node (ref U2) (pin 6))
      (node (ref J2) (pin 4)))
    (net (code 21) (name "Net-(J2-Pad2)")
      (node (ref U2) (pin 4))
      (node (ref J2) (pin 2)))
    (net (code 22) (name +5V)
      (node (ref U3) (pin 3))
      (node (ref U2) (pin 39))
      (node (ref C2) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 23) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6))
      (node (ref U2) (pin 9)))
    (net (code 24) (name SCK)
      (node (ref U2) (pin 24))
      (node (ref U1) (pin 12)))
    (net (code 25) (name NSS)
      (node (ref U1) (pin 15))
      (node (ref U2) (pin 11)))
    (net (code 26) (name MISO)
      (node (ref U1) (pin 13))
      (node (ref U2) (pin 21)))
    (net (code 27) (name MOSI)
      (node (ref U2) (pin 25))
      (node (ref U1) (pin 14)))
    (net (code 28) (name "Net-(Q1-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 29) (name DIO0)
      (node (ref U2) (pin 14))
      (node (ref U1) (pin 5)))
    (net (code 30) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 31) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 32) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 33) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 34) (name "Net-(U2-Pad43)")
      (node (ref U2) (pin 43)))
    (net (code 35) (name "Net-(U2-Pad42)")
      (node (ref U2) (pin 42)))
    (net (code 36) (name "Net-(U2-Pad41)")
      (node (ref U2) (pin 41)))
    (net (code 37) (name "Net-(U2-Pad40)")
      (node (ref U2) (pin 40)))
    (net (code 38) (name "Net-(U2-Pad20)")
      (node (ref U2) (pin 20)))
    (net (code 39) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 40) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 41) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 42) (name "Net-(U2-Pad22)")
      (node (ref U2) (pin 22)))
    (net (code 43) (name "Net-(U2-Pad30)")
      (node (ref U2) (pin 30)))
    (net (code 44) (name "Net-(U2-Pad37)")
      (node (ref U2) (pin 37)))
    (net (code 45) (name "Net-(U2-Pad36)")
      (node (ref U2) (pin 36)))
    (net (code 46) (name "Net-(U2-Pad35)")
      (node (ref U2) (pin 35)))
    (net (code 47) (name "Net-(U2-Pad34)")
      (node (ref U2) (pin 34)))
    (net (code 48) (name "Net-(U2-Pad33)")
      (node (ref U2) (pin 33)))
    (net (code 49) (name "Net-(U2-Pad29)")
      (node (ref U2) (pin 29)))
    (net (code 50) (name "Net-(U2-Pad27)")
      (node (ref U2) (pin 27)))
    (net (code 51) (name "Net-(U2-Pad26)")
      (node (ref U2) (pin 26)))))